Procedure for handling and disposal of isolated Asbestos pieces.

Site Address: Edgecumbe

The following PPE should be worn **at all times** by workers on any site where asbestos pieces are suspected and to be handled to minimise the risk of breathing in asbestos. (This procedure applies to material involving less than an equivalent of 10m2) If over 10m2 of material requires removal specialist contractors and notification is required.

PPE must include:

* Respiratory protective equipment (P2 mask) – to avoid inhaling asbestos fibres.
* Disposal gloves.
* Overalls which are impervious to asbestos dust (disposable hooded coveralls) – to avoid the risk of carrying asbestos fibres away from the worksite on clothing

Such amounts shall be collected and placed in 200 micron thick yellow plastic “Contaminated Waste bags” with “ASBESTOS” written across them.

The sealed bags shall be dropped off to Waste Management Technical Services at 31 Gateway Drive, Whakatāne . They have limited opening hours as the team are often out and about, but they are open Mon and Thu from 7.30 to 4.30 when the office lady is present. It is best to call Paul Thurman the site manager on 0275 264 239 to check they are open. Weighed bags shall be invoiced to WDC with a PO number obtain from Pearl at the Liveable Homes office.

Name of Contractor

Signed by Contractor

Dated